Write a config file so that wpa\_supplicant can associate to FT Dot1x WLAN

ctrl\_interface=/var/run/wpa\_supplicant

update\_config=1

network={

ssid="Airtel\_chen\_9369"

proto=RSN

key\_mgmt=FT-EAP

pairwise=CCMP

group=CCMP

eap=PEAP

identity="admin"

password="admin"

phase2="auth=MSCHAPV2"

phase1="peaplabel=1 peapver=0"

priority=1

}